Switch#show running-config

Building configuration...

Current configuration : 1778 bytes

!

version 12.2(37)SE1

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname Switch

!

!

!

!

!

!

ip routing

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

spanning-tree mode pvst

spanning-tree vlan 40,50 priority 24576

!

!

!

!

!

!

interface Port-channel1

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface FastEthernet0/1

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface FastEthernet0/2

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface FastEthernet0/3

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface FastEthernet0/4

switchport trunk encapsulation dot1q

switchport mode trunk

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

switchport trunk encapsulation dot1q

switchport mode trunk

channel-group 1 mode on

!

interface FastEthernet0/23

switchport trunk encapsulation dot1q

switchport mode trunk

channel-group 1 mode on

!

interface FastEthernet0/24

switchport trunk encapsulation dot1q

switchport mode trunk

channel-group 1 mode on

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

shutdown

!

ip classless

!

ip flow-export version 9

!

!

!

!

!

!

!

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

!

!

!

end