!

!

interface FastEthernet0/0

ip address 2.2.2.1 255.255.255.0

duplex auto

speed auto

!

interface FastEthernet0/1

ip address 3.3.3.1 255.255.255.0

duplex auto

speed auto

!

interface Serial0/1/0

no ip address

encapsulation frame-relay

!

interface Serial0/1/0.10 point-to-point

ip address 10.1.1.2 255.255.255.252

frame-relay interface-dlci 201

clock rate 2000000

!

interface Serial0/1/0.30 point-to-point

ip address 10.1.1.5 255.255.255.252

frame-relay interface-dlci 203

clock rate 2000000

!

interface Serial0/1/1

no ip address

clock rate 2000000

!

interface Vlan1

no ip address

shutdown

!

router ospf 1

log-adjacency-changes

network 10.1.1.0 0.0.0.3 area 0

network 10.1.1.4 0.0.0.3 area 0

network 2.2.2.0 0.0.0.255 area 0

network 3.3.3.0 0.0.0.255 area 0

!

ip classless

!

ip flow-export version 9

!

!

!

!

!

!

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

!

!