Door

Open / Close / Unlock / Lock

Features:

* Registration Server Compatible
* Ability to vent Carbon Dioxide and Carbon Monoxide

Usage:

* Connect to the Door from SBC/MCU/Thing with IoT Custom Cable
* Use customWrite function to control the door and lock

Direct Control:

* ALT-click on keyhole to lock/unlock
* ALT-click on door to open/close

Local Control:

* Connect device to SBC/MCU/Thing. Use the "customWrite" API per Data Specifications

Remote Control:

* Connect device to Registration Server using Config Tab

NOTE: opening and closing the door is not remote controllable

Data Specifications:

Message Format: [door],[lock]

door: 0 = closed, 1 = open, -1 = don't care

lock: 0 = unlock, 1 = lock, -1 = don't care

Example:

Connect a SBC to the door, send a customWrite and open the door to vent the Carbon Dioxide and Carbon Monoxide level