Window

A window that can open or close

Features:

* Registration Server Compatible
* Ability to vent Carbon Dioxide and Carbon Monoxide

Usage:

* Window works with Environment object. It reads CARBON\_DIOXIDE and CARBON\_MONOXIDE variables set in the Environment object and change these variables when users activate window opening/closing

Direct Control:

* ALT-click to open and close

Local Control:

* Connect device to MCU/SBC/Thing. Use the "customWrite" API per Data Specifications

Remote Control:

* Connect device to Registration Server using Config Tab

Data Specifications:  
Message Format: [state]  
state: 0 = closed, 1 = open

Example:

* N/A