Router#show running-config

Building configuration...

Current configuration : 1004 bytes

!

version 15.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname Router

!

!

!

!

!

!

!

!

no ip cef

no ipv6 cef

!

!

!

!

license udi pid CISCO2811/K9 sn FTX1017745T-

!

!

!

!

!

!

!

!

!

!

!

spanning-tree mode pvst

!

!

!

!

!

!

interface FastEthernet0/0

ip address 6.6.6.1 255.255.255.0

duplex auto

speed auto

!

interface FastEthernet0/1

ip address 4.4.4.1 255.255.255.0

duplex auto

speed auto

!

interface Serial0/1/0

ip address 10.1.1.1 255.255.255.252

encapsulation frame-relay

frame-relay interface-dlci 102

ip ospf network point-to-point

ip ospf priority 1

!

interface Serial0/1/1

no ip address

clock rate 2000000

shutdown

!

interface Vlan1

no ip address

shutdown

!

router ospf 1

log-adjacency-changes

network 10.1.1.0 0.0.0.3 area 0

network 4.4.4.0 0.0.0.255 area 0

network 6.6.6.0 0.0.0.255 area 0

!

ip classless

!

ip flow-export version 9

!

!

!

!

!

!

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

!

!

end