Switch#show running-config

Building configuration...

Current configuration : 1713 bytes

!

version 15.0

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname Switch

!

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

switchport mode trunk

!

interface FastEthernet0/2

switchport mode trunk

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

switchport access vlan 10

switchport mode access

!

interface FastEthernet0/7

switchport access vlan 10

switchport mode access

!

interface FastEthernet0/8

switchport access vlan 10

switchport mode access

!

interface FastEthernet0/9

switchport access vlan 20

switchport mode access

!

interface FastEthernet0/10

switchport access vlan 20

switchport mode access

!

interface FastEthernet0/11

switchport access vlan 20

switchport mode access

!

interface FastEthernet0/12

switchport access vlan 30

switchport mode access

!

interface FastEthernet0/13

switchport access vlan 30

switchport mode access

!

interface FastEthernet0/14

switchport access vlan 30

switchport mode access

!

interface FastEthernet0/15

switchport access vlan 40

switchport mode access

switchport voice vlan 50

!

interface FastEthernet0/16

switchport access vlan 40

switchport mode access

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

shutdown

!

!

!

!

line con 0

!

line vty 0 4

login

line vty 5 15

login

!

!

!

!

endb