!

interface FastEthernet0/0

ip address 6.6.6.2 255.255.255.0

ip access-group 100 out

duplex auto

speed auto

!

interface FastEthernet0/1

no ip address

duplex auto

speed auto

!

interface FastEthernet0/1.15

encapsulation dot1Q 15

ip address 192.168.15.2 255.255.255.0

ip access-group 115 in

standby 3 ip 192.168.15.1

standby 3 priority 200

standby 3 preempt

!

interface FastEthernet0/1.25

encapsulation dot1Q 25

ip address 192.168.25.2 255.255.255.0

ip access-group 125 in

standby 3 ip 192.168.25.1

standby 3 priority 200

standby 3 preempt

!

interface FastEthernet0/1.35

encapsulation dot1Q 35

ip address 192.168.35.2 255.255.255.0

ip access-group 135 in

standby 3 ip 192.168.35.1

standby 3 priority 150

standby 3 preempt

!

interface FastEthernet0/1.45

encapsulation dot1Q 45

ip address 192.168.45.2 255.255.255.0

ip access-group 145 in

standby 3 ip 192.168.45.1

standby 3 priority 150

standby 3 preempt

!

interface FastEthernet0/1.55

encapsulation dot1Q 55

ip address 192.168.55.2 255.255.255.0

standby 3 ip 192.168.55.1

standby 3 priority 150

standby 3 preempt

!

interface Vlan1

no ip address

shutdown

!

router ospf 1

log-adjacency-changes

network 6.6.6.0 0.0.0.255 area 0

network 192.168.15.0 0.0.0.255 area 0

network 192.168.25.0 0.0.0.255 area 0

network 192.168.35.0 0.0.0.255 area 0

network 192.168.45.0 0.0.0.255 area 0

network 192.168.55.0 0.0.0.255 area 0

!

ip classless

!

ip flow-export version 9

!

!

access-list 100 permit udp any host 192.168.99.3 eq domain

access-list 100 permit tcp 192.168.35.0 0.0.0.255 host 192.168.99.4 eq www

access-list 100 permit ip 192.168.45.0 0.0.0.255 host 192.168.99.4

access-list 100 permit ip any host 192.168.99.5

access-list 100 permit tcp any host 192.168.99.6 eq pop3

access-list 100 permit tcp any host 192.168.99.6 eq smtp

access-list 100 permit tcp any host 192.168.99.7 eq www

access-list 100 permit tcp any host 192.168.99.7 eq 443

access-list 100 permit tcp any 8.8.8.0 0.0.0.255 eq 443

access-list 100 permit ip 192.168.55.0 0.0.0.255 192.168.6.0 0.0.0.255

access-list 100 permit ip 192.168.55.0 0.0.0.255 192.168.50.0 0.0.0.255

access-list 100 permit icmp 192.168.45.0 0.0.0.255 192.168.5.0 0.0.0.255

access-list 100 permit icmp 192.168.45.0 0.0.0.255 192.168.40.0 0.0.0.255

access-list 100 deny ip any any

access-list 145 permit icmp any 192.168.45.0 0.0.0.255

access-list 145 deny ip any 192.168.15.0 0.0.0.255

access-list 145 deny ip any 192.168.25.0 0.0.0.255

access-list 145 deny ip any 192.168.35.0 0.0.0.255

access-list 145 permit ip any any

access-list 125 permit icmp any 192.168.25.0 0.0.0.255

access-list 125 deny ip any 192.168.15.0 0.0.0.255

access-list 125 deny ip any 192.168.35.0 0.0.0.255

access-list 125 deny ip any 192.168.45.0 0.0.0.255

access-list 125 permit ip any any

access-list 115 permit icmp any 192.168.15.0 0.0.0.255

access-list 115 deny ip any 192.168.25.0 0.0.0.255

access-list 115 deny ip any 192.168.35.0 0.0.0.255

access-list 115 deny ip any 192.168.45.0 0.0.0.255

access-list 115 permit ip any any

access-list 135 permit icmp any 192.168.35.0 0.0.0.255

access-list 135 deny ip any 192.168.15.0 0.0.0.255

access-list 135 deny ip any 192.168.25.0 0.0.0.255

access-list 135 deny ip any 192.168.45.0 0.0.0.255

access-list 135 permit ip any any

!

no cdp run

!

!

!

!

!

dial-peer voice 77 voip

destination-pattern 300.

session target ipv4:3.3.3.2

!

dial-peer voice 200 voip

destination-pattern 200.

session target ipv4:5.5.5.2

!

dial-peer voice 400 voip

destination-pattern 300.

session target ipv4:2.2.2.2

!

dial-peer voice 500 voip

destination-pattern 200.

session target ipv4:1.1.1.2

!

telephony-service

max-ephones 10

max-dn 15

ip source-address 192.168.55.1 port 2000

!

ephone-dn 1

number 4001

!

ephone-dn 2

number 4002

!

ephone-dn 3

number 4003

!

ephone-dn 4

number 4004

!

ephone 1

device-security-mode none

mac-address 0001.42A1.9B68

type 7960

button 1:1

!

ephone 2

device-security-mode none

mac-address 0001.96B6.DE2D

type 7960

button 1:2

!

ephone 3

device-security-mode none

mac-address 0040.0B61.6AC6

type 7960

button 1:3

!

ephone 4

device-security-mode none

mac-address 0030.F238.116D

type 7960

button 1:4

!

line con 0

!

line aux 0

!

line vty 0 4

login

!

!

!

end