Blower

Blower Fan

Features:

* Registration Server Compatible
* Off
* Low Speed
* High Speed

Usage:

* Connect to the Blower with custom cable from MCU/SBC/Thing
* In the script, write the data to the Blower with customWrite function to turn Blower off, set low speed/high speed

Direct Control:

* ALT-click to interact

Local Control:

* Connect device to MCU/Thing/SBC. Use the "customWrite" API per Data Specifications

Remote Control:

* Connect device to Registration Server using Config Tab

Data Specifications:

Message Format: [state]

state: 0 = off, 1 = low speed, 2 = high speed

Example:

Connect SBC to a Blower with custom cable, connect from pin 0 on SBC to pin 0 on the Blower, in the SBC, add the code customWrite(0, "1") to set the Blower at low speed